# **|** **Suggested Specifications | Section 10 19 00**

# **Vinyl Shower Curtains**

**Part 1 – General**

* 1. **Related Documents**
1. Drawings and general provisions of the Contract, including General and Supplementary Conditions and Division 1 Specification Sections, apply to this Section.

	1. **Summary**
2. This section includes the following:
3. Vinyl shower curtains

**1.03 Performance Requirements**

1. Curtains: Provide curtain fabrics with the following characteristics:
2. Fabrics are flame resistant and are identical to those that have passed NFPA 701 when tested by a testing and inspecting agency acceptable to authorities having jurisdiction (AHJ).

	1. **Submittals**
3. Product Data: Submit copies of manufacturer’s detailed technical data for materials, fabrication, and physical appearance.
4. Shop Drawings: Show layout and types of cubicle curtains, sizes of curtains, and number of carriers.
5. Samples for Verification: Provide samples of the following
6. Curtain Fabric: 12-inch square swatch or larger sample as required to show complete pattern repeat, from dye lot used for the work, with specified treatments applied.

	1. **Warranty**
7. Provide copy of manufacturer’s standard warranty.

**Part 2 - Products**

**2.01 Manufacturers**

1. Subject to compliance with the requirements listed, provide cubicle curtains from the following manufacturer:
2. CS Cubicle Curtains, a Division of Construction Specialties, Inc.

3 Werner Way

Lebanon, NJ 08833

P: (800) 416 - 1102

CCInfo@c-sgroup.com

www.c-sgroup.com

1. Alternative manufacturers will not be accepted

**2.02 Materials**

1. Shower Curtain:
2. Fabric: Fabric to be vinyl, intrinsically fire retardant, and antimicrobial.

**2.03 Pattern and Color**

<\*\*Note to specifier – please select one of the following standard colors for shower curtains>

1. Shower Curtain Fabric: Fabric to be CS Sure-Check linen fabric in the following color:
2. Light Blue
3. Bordeaux
4. Dune
5. Mint
6. Muave
7. Fawn
8. Yellow
9. Translucent
10. White
11. Seafoam

**2.04 Fabrication**

1. Shower Curtains to be fabricated as follows:
2. Width: Equal to track (or shower curtain rod) length from which curtain is hung plus 10 percent, but not less than 12" (300 mm).
3. Length: Equal to floor-to-ceiling (or shower rod-to-floor) height minus 2" from finished ceiling at top and 1" above finished floor.
4. Top Hem: Not less than 1" (26 mm) and not more than 1 ½" (40 mm) wide, triple thickness, reinforced with integral web and double stitched.
	1. Grommets: 2 piece, rolled-edge, rustproof, nickel-plated brass and spaced not more than 6" (150 mm) o.c.
5. Bottom and Side Hems: Not less than 1" (25 mm) wide, reinforced, triple thickness and single stitched.
6. Seams: Not less than ½" (13 mm) wide, double turned and double stitched.
7. Curtain Tieback: At each termination.

**Part 3 – Execution**

**3.01 Examination**

1. Examine areas and conditions in which the cubicle track system will be installed

**1**. Complete all finishing operations, including painting, before beginning installation of cubicle tracking system materials.

1. Verify that surfaces and above ceiling supports are ready to receive work.

**3.02 Cleaning**

1. At completion of the installation, remove any debris and clean surfaces in accordance with CS cleaning and maintenance instructions.

END OF SECTION