Hookless Shower Curtains

Suggested Specifications | Section 10 21 23

**Part 1 – General**

* 1. **Related Documents**
1. Drawings and general provisions of the Contract, including General and Supplementary Conditions and Division 1 Specification Sections, apply to this Section.

	1. **Summary**
2. This section includes the following:
3. Hookless shower curtains

**1.03 Performance Requirements**

1. Curtains: Provide curtain fabrics with the following characteristics:
2. Polyester fabrics are launderable at temperatures of 140 degrees F (60 Deg C).
3. CS does not recommend washing vinyl shower curtains in a washing machine. Instead, vinyl curtains should be wiped down with warm, soapy water and then thoroughly rinsed. Allow the curtain to completely air dry before next use (if possible).

	1. **Submittals**
4. Product Data: Submit copies of manufacturer’s detailed technical data for materials, fabrication, and physical appearance.
5. Shop Drawings: Show layout and types of cubicle curtains, sizes of curtains, and number of carriers.
6. Samples for Verification: Provide samples of the following:
7. Curtain Fabric: 12-inch square swatch or larger sample as required to show complete pattern repeat, from dye lot used for the work, with specified treatments applied.

	1. **Warranty**
8. Provide copy of manufacturer’s standard warranty.

**Part 2 - Products**

* 1. **2.01 Manufacturer**

**A. Basis of Design - m**anufactured by Construction Specialties Subject to compliance with the requirements listed, provide cubicle curtains from the following manufacturer:

Construction Specialties, 3 Werner Way, Lebanon, NJ 08833. Tel: 800.233.8493. Email: cet@c-sgroup.com No substitutions.

**B**. Drawings and specifications are based on manufacturer’s literature from Construction Specialties, Inc. drawings and specifications unless otherwise indicated. Other manufacturers must be approved equal by Architect/Owner.

**2.02 Materials**

1. Shower Curtain:
2. Fabric: Fabric to be non-vinyl, and antimicrobial.

**2.03 Pattern and Color**

<\*\*Note to specifier – please select one of the following standard colors for Hookless shower curtains>

1. Shower Curtain Fabric: Fabric in the following pattern/color:
	1. Pin Dot (Eight Gauge Vinyl).

**1)** Color: Beige – Size: 42” x 74”

**2)** Color: White - Sizes: 71” x 80”, 71” x 74” or 42” x 74”

* 1. Litchfield (100% Polyester)

**1)** Color: White – Sizes: 71” x 74” or 42´x 74”

**2)** Color: Beige – Sizes: 71” x 74” or 42” x 74”

* 1. Mini-Square (100% Polyester, Fire Retardant, meets NFPA 701))

**1)** Color: Beige. Sizes: 42” x 74” or 71” x 74”

**2)** Color: Sage Size: 42” x 74”

* 1. Mystery with Sheer Window (100%Polyester)

**1)** Color: White – Size: 71’ x 74”

**2)** Color: Beige – Size: 71” x 74”

**3)** Color: Sage – Size: 71” x 74”

**2.04 Fabrication**

1. Shower Curtains to be fabricated as follows:

**a)** Panel Size:

**1)** 71” x 74”

 **2**) 42” x 74”

  **3)** Custom: \_\_\_\_\_\_\_\_

**Part 3 – Execution**

**3.01 Examination**

1. Examine areas and conditions in which the shower curtain will be installed

**1.** Complete all finishing operations, including painting, before beginning installation of shower curtain and curtain rod/track materials.

1. Verify that surfaces and above ceiling supports are ready to receive work.

**3.02 Cleaning**

1. At completion of the installation, remove any debris and clean surfaces in accordance with CS cleaning

and maintenance instructions.

END OF SECTION