**SUGGESTED CANADIAN SPECIFICATIONS**

**SECTION 10 26 00**

**C/S Acrovyn® 4000 .040N Rigid Sheet**

# Part 1 - General 1.01 Summary

1. This section includes the following types of wall protection systems:
   1. Wall Covering
2. Related sections: The following sections contain requirements related to this section:
   1. Handrails, Bumper Guards, Crash Rails, Corner Guards, Accent Rails, Wall Panels, Door Protection; refer to section 10 26 00 “Wall and Door Protection”

# 1.02 References

1. National Building Code of Canada, “NBC” (2010)
2. National codes (IBC, UBC, SBCCI, BOCA, Life Safety and CA 01350)
3. American Society for Testing and Materials (ASTM)
4. Underwriters Laboratories (UL)
5. California 01350 specification

# 1.03 Submittals

1. General: Submit the following in accordance with conditions of contract and Division 1 specification section 01 33 00 “Submittal Procedures”.
2. Product data and detailed specifications for each system component and installation accessory required, including installation methods for each type of substrate.
3. Shop drawings showing locations, extent and installation details of wall covering products.
4. Samples for verification purposes: Submit the following samples, as proposed for this work, for verification of color, texture, pattern and thickness:

**1.** Sample of each product specified.

1. Product test reports from a qualified independent testing laboratory showing compliance of each component with requirements indicated.
2. Maintenance data for wall protection system components for inclusion in the operating and maintenance manuals specified in Division 1.

# 1.04 Quality Assurance

1. Installer qualifications: Engage an installer who has no less than 3 years experience in installation of systems similar in complexity to those required for this project.
2. Manufacturer’s qualifications: Not less than 5 years experience in the production of specified products and a record of successful in-service performance.
3. Code compliance: Assemblies should conform to all applicable codes including NBC (2010), IBC, UBC, SBCCI, BOCA, Life Safety and CA 01350.
4. Fire performance characteristics: Provide engineered PETG wall protection system components tested to Canadian Required CAN/ULC S102.2, “Test for Surface Burning Characteristics of Flooring, Floor Coverings, and Miscellaneous Materials and Assemblies” with results listed below:
   1. Flame spread: 150 or less
   2. Smoke developed: 300 or less
5. Impact Strength: Provide assembled wall protection units that have been tested in accordance with the applicable provisions of ASTM F476.
6. Chemical and stain resistance: Provide wall protection system components with chemical and stain resistance in accordance with ASTM D543.
7. Color match: Provide wall protection components that are color matched in accordance with the following:
   1. Delta Ecmc of no greater than 1.0 using CIELab color space. (Specifier note: Construction Specialties’ colors are matched under cool white fluorescent lighting and computer controlled within manufacturing tolerances. Color may vary if alternate lighting sources are present).
8. Single source responsibility: Provide all components of the wall protection system manufactured by the same company to ensure compatibility of color, texture and physical properties.

# 1.05 Delivery, Storage and Handling

1. Deliver materials to the project site in unopened original factory packaging clearly labeled to show manufacturer.
2. Store materials in original, undamaged packaging in a clean, dry place out of direct sunlight and exposure to the elements. A minimum room temperature of 40ºF (4ºC) and a maximum of 100ºF (38ºC) should be maintained. **C.** Materials must be stored flat.

# 1.06 Project Conditions

1. Materials must be acclimated in an environment of 65-75ºF (18-24ºC) for at least 24 hours prior to beginning the installation.
2. Installation areas must be enclosed and weatherproofed before installation commences.

# Part 2 - Products 2.01 Manufacturers

**A.** Interior surface protection products specified herein and installed on the submittal drawings shall be manufactured by Construction Specialties, Inc.

# 2.02 Materials

**A.** Engineered PETG: Rigid sheet should be high impact Acrovyn 4000 with nominal .040" (1.02mm) thickness and supplied in 4' x 8' or 10' (1.22m x 2.44m or 3.05m) sheet sizes in standard Suede texture. Quatro, Single Tread, Beadboard (specify nominal 1-5/8" or 2-5/8"), Mesa, Stone Chips, Irish Linen, Pindot, Leather, Pinstripe, Dado and Stipple textures shall be 43" x 90" or 114" (1.09m x 2.29m or 2.90m). Select from one of (64)\* Acrovyn solid colors or (18)\* Chameleon patterned colorways which include (16) woodgrains and (2) metals. Specify color-matched caulk, plastic trims or metal trims as needed for joints/transitions. (\*Specifier note: refer to color selectors to determine which colors and patterns are *Cradle to Cradle CertifiedCM* Gold or Silver.)

# 2.03 Fabrication

**A.** General: Fabricate wall covering to comply with requirements indicated for design, dimensions, detail, finish and sizes.

# 2.04 Accessories

**A.** Acrovyn Wall Covering shall be furnished as a complete packaged system, containing all adhesive. Adhesive shall be water based and non-hazardous. Water based primer is also available for purchase.

# Part 3 - Execution 3.01 Examination

**A.** Verification of conditions: Examine areas and conditions under which work is to be performed and identify conditions detrimental to proper or timely completion.

1. Do not proceed until unsatisfactory conditions have been corrected.
2. PVC-Free Materials to be installed only as permitted per local building codes.

# 3.02 Preparation

1. Surface preparation: Prior to installation, clean substrate to remove dirt, debris and loose particles. Perform additional preparation procedures as required by manufacturer's instructions.
2. Protection: Take all necessary steps to prevent damage to material during installation as required in manufacturer's installation instructions.

# 3.03 Installation

1. Install the work of this section in strict accordance with the manufacturer's recommendations using approved adhesive.
2. Temperature at the time of installation must be between 65-75ºF (18-24ºC) and be maintained for at least 48 hours after the installation to allow for proper adhesive set up.
3. Relative humidity shall not exceed 80%.
4. Do not expose wall covering to direct sunlight during or after installation. This will cause the surface temperature to rise, which in turn will cause bubbles and delamination.

# 3.04 Cleaning

1. General: Immediately upon completion of installation, clean wall covering and accessories in accordance with manufacturer's recommended cleaning method.
2. Remove surplus materials, rubbish and debris resulting from installation as work progresses and upon completion of work.

# 3.05 Protection

**A.** Protect installed materials to prevent damage by other trades. Use materials that may be easily removed without leaving residue or permanent stains.